|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| SL NO. | PART NAME | MATERIAL WITH WHICH THE PART IS MADE UP OF | DESCRIPTION  ABOUT PART | QUANTITY REQUIRED | FABRICATION REQUIRED |
| 1 | OUTER BODY | ACRYLIC SHEET | SHEET MADE OF ACRYLIC FIBRE | 6 FEET | BENDING AND CUTTING |
| 2 | USB CABLES | MADE OF WIRES OF COPPER | USED TO CONNECT ELECTRONICS USE THE PROTOCOL | 02 | \_ |
| 3 | WATER PUMP | \_ | V--2-3V | 01 | \_ |
| 4 | OHM RESISTOR | MADE OF INSULATING MATERIAL,USUALLY CERAMIC | --1KOHMS-- | 01 | \_ |
| 5 | IR SENSOR | \_ | V-5Vdetection  Distance 1-2cm | 01 | \_ |
| 6 | MINI SWITCH | MADE OF PORCELAIN | ---- | 01 | \_ |
| 7 | TRANSISTOR  T 1P H2 C | \_ | CURRENT -6A  THE BASE HAS-3A | 01 | \_ |
| 8 | TRANSPARENT PIPE | FIBER | TRANSFERS THE OINTMENT | 01 | \_ |
| 9 | PLASTIC BOTTLE | PLASTIC | USED FOR STORAGE OF OINTMENT | 01 | \_ |